303(d) Listing Documentation

Waterbody Name:  Kummel Creek
Waterbody ID Code (WBIC):  863500
County (ies): Fond du Lac, Dodge
Impaired Stream Reach: 0 – 11.54 miles
Type of impairment (water quality standards violations [eg, pH, DO, etc.], not meeting codified use [e.g. WWFF should be Cold II], eutrophication, etc.]:
Dissolved Oxygen
Cause of impairment (e.g. temperature, nutrients, sediment, BOD, toxics, etc.):
Nutrients
Source of impairment (e.g. point source, nonpoint source, internal load, unknown, etc.):
Point and nonpoint sources
Description of monitoring conducted (including dates, results, quality of data and reports):   Fixed period baseflow and runoff event samples collected at HWY 67 and analyzed for Dissolved P, TP, N, and Kjeldahl N from June 2004 through November 2005.  Four samples were collected at various crossings upstream of HWY 67 during baseflow conditions in 2005 and were also analyzed for nutrients.  Elevated nutrient levels are found at the downstream crossings nearest to the point sources ( HH & Center Rd.) compared to samples collected above the point sources and samples collected at sites further downstream.
Weeklong hydrolab deployments were done seasonally from June 2004 – November 2005 between Hwy 49 and Hwy 67 to monitor dissolved oxygen.  Not enough summer data has been collected so Horicon staff will continue hydrolab deployments in the summer of 2006.
Location of supporting data (electronic and hard copy files): 
Watershed file share under TMDL Monitoring folder.  
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